Home Contents | # v4kf:chipDisable | V4kf | Core4 Lua Event System

## SYNOPSIS

rdrhandle:chipDisable()

## DESCRIPTION

Disables a chip card. Power to the chip is turned off.

This command can only be used if the reader is in the Locked state, which secures the chip card against removal during operation.

While this state processes, the reader is in the Processing state and v4kf:isProcessing() returns true. The reader returns to the Locked state on completion.

The command returns immediately. Actual execution of any reader operation is done within the event loop.

The processing result is provided with the v4kf.processingComplete() callback.

## SEE ALSO

v4kf:chipEnable, v4kf:chipRead, v4kf:chipWrite, v4kf:chipIdentify, v4kf:state