Home Contents | # New BiS handler | Bis | Core4 Lua Event System

## SYNOPSIS

1. bishandle = bis.newmaster(app, devicename_or_handle [, speed])
2. bishandle = bis.newslave(app, devicename_or_handle [, speed])
3. bishandle:close()

## DESCRIPTION

Create a new BiS event handler. The handler is attached to the event processor passed in app.

If a string is passed as second parameter devicename_or_handle, this must be the device name of a serial port, the optional speed parameter selects the port speed, which defaults to 115200bps.

Passing a file handle as second parameter allows using an already open handle, for example a network connection. When the file handle is a serial port, it is automatically configured for BiS (8N1), including the optional speed parameter. When no speed is given, the port speed is not changed.

The bis:close() will close the handle when no longer needed. The BiS handle becomes invalid. This automatically happens during garbage collection, but that takes an unknown amount of time. A serial port is closed only if it was opened by the BiS code.

## RETURN VALUE

On success, a BiS event handler instance. On failure, three values are returned: nil, a string describing the error (The result of the C library call strerror() on the errno code) and the errno number from the standard C library.

## EXAMPLE

> >
app = event.new() bis = bis.newmaster(app, "/dev/ttyS1", 38400)

## SEE ALSO

bis:setAddress, bis:address, bis:setSeqNr, bis:seqNr, bis:send, bis.receive, bis.receiveMTD16