Home Contents | # gpio.info | Gpio | Core4 Lua Event System

## SYNOPSIS

#include <lua/gpio.lh>
gpio.info(group)

## DESCRIPTION

Query information about a gpio group. The group is either one of the GPGRP_xxx values defined in lua/gpio.lh or a registered ID used with gpio.register().

The result is a table with information about the group or device. A field is only present in the table if that information is available.

parent | The parent group number. For example GPGRP_MUPP for multi-io devices talking MUPP protocol.
address | The address on the bus.
device | The serial device where the bus is attached to.
state | Either "up" or "down", indicating if the device is responding.
type | A code number indicating the type of the device.
capabilities | Capability flag bits.
version | Version number of the device firmware.
name | The type name of the device in UTF8 encoding. For example "eemio" or "µMIO".
ttycount | Number of tunneled serial ports.

## RETURN VALUE

On success, returns a table. On error, three values are returned: nil, a string describing the error (The result of the C library call strerror() on the errno code) and the errno number from the standard C library.

## SEE ALSO

gpio.register, gpio.unregister, gpio.read, gpio.write