Home Contents | # bis:address | Bis | Core4 Lua Event System

## SYNOPSIS

1. addr = bishandle:address()
2. bishandle:setAddress(addr)

## DESCRIPTION

### Master mode

These functions have no useful purpose in master mode.

### Slave mode

The first form returns the configured slave address, while the second form allows configuring a slave address.

## RETURN VALUE

The first form returns the slave address as a number.

## NOTES

The BiS protocol supports slave addresses of up to 32 bits. Some smaller devices support only 8 bit addressing, though.