Home Contents | # v4kf.processingComplete | V4kf | Core4 Lua Event System

## SYNOPSIS

rdrhandle.processingComplete = function(rdrhandle, res [, data])

## DESCRIPTION

This callback is run whenever a chip card access completes. res is zero on success and contains an error code on error. If the chip access has provided some data (e.g. v4kf:chipRead()), then the data parameter is a string containing the data.

## BUGS

The res parameter needs to be explained.

## SEE ALSO

v4kf:chipRead, v4kf:chipWrite, v4kf:chipExecute, v4kf:clearCallbacks, v4kf.magdataChanged, v4kf.stateChanged, v4kf:state